*** Creating Trace Output File 'SSD1928L 8BIT Demo.tra' Ok.
### Preparing for ADS-LD.
### Creating ADS-LD Command Line
### List of Objects: adding '"startup.o"'
### List of Objects: adding '"ssd1928l demo.o"'
### List of Objects: adding '"system.o"'
### List of Objects: adding '"ssd1928l_8bit.o"'
### List of Objects: adding '"tmr0.o"'
### ADS-LD Command completed:
"startup.o" "ssd1928l demo.o" "system.o" "ssd1928l_8bit.o" "tmr0.o" --device DARMP --strict --scatter "SSD1928L 8BIT Demo.sct" 

--autoat --summary_stderr --info summarysizes --map --xref --callgraph --symbols 

--info sizes --info totals --info unused --info veneers 

 --list ".\SSD1928L 8BIT Demo.map" -o "SSD1928L 8BIT Demo.axf"### Preparing Environment (PrepEnvAds)
### ADS-LD Output File: 'SSD1928L 8BIT Demo.axf'
### ADS-LD Command File: 'SSD1928L 8BIT Demo.lnp'
### Checking for dirty Components...
### Creating CmdFile 'SSD1928L 8BIT Demo.lnp', Handle=0x00000404
### Writing '.lnp' file
### ADS-LD Command file 'SSD1928L 8BIT Demo.lnp' is ready.
### ADS-LD: About to start ADS-LD Thread.
### ADS-LD: executed with 0 errors
### Updating obj list
### LDADS_file() completed.
