!_TAG_FILE_FORMAT	2	/extended format; --format=1 will not append ;" to lines/
!_TAG_FILE_SORTED	1	/0=unsorted, 1=sorted, 2=foldcase/
!_TAG_PROGRAM_AUTHOR	Darren Hiebert	/dhiebert@users.sourceforge.net/
!_TAG_PROGRAM_NAME	Exuberant Ctags	//
!_TAG_PROGRAM_URL	http://ctags.sourceforge.net	/official site/
!_TAG_PROGRAM_VERSION	5.5.4	//
!_TAG_REVISION_NAME	MCHPTags	//
!_TAG_REVISION_VERSION	6.0.1	//
BOOLEAN	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\HY27US08561A\HY27US08561A.h	43;"	t	line:43
DeviceID	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\mainDemo.c	47;"	v	line:47
HIGH::1	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\HY27US08561A\HY27US08561A.h	79;"	d	line:79
INPUT::1	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\HY27US08561A\HY27US08561A.h	76;"	d	line:76
INT16U	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\HY27US08561A\HY27US08561A.h	42;"	t	line:42
INT8U	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\HY27US08561A\HY27US08561A.h	41;"	t	line:41
LOW::0	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\HY27US08561A\HY27US08561A.h	78;"	d	line:78
NAND_ALE_LAT::LATDbits.LATD11	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\HY27US08561A\HY27US08561A.h	69;"	d	line:69
NAND_ALE_TRIS::TRISDbits.TRISD11	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\HY27US08561A\HY27US08561A.h	68;"	d	line:68
NAND_BLOCKERASE_C1::0x60	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\HY27US08561A\HY27US08561A.h	95;"	d	line:95
NAND_BLOCKERASE_C2::0xD0	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\HY27US08561A\HY27US08561A.h	96;"	d	line:96
NAND_BLOCK_COUNT::2048	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\HY27US08561A\HY27US08561A.h	106;"	d	line:106
NAND_CE_LAT::LATGbits.LATG12	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\HY27US08561A\HY27US08561A.h	65;"	d	line:65
NAND_CE_TRIS::TRISGbits.TRISG12	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\HY27US08561A\HY27US08561A.h	64;"	d	line:64
NAND_CLE_LAT::LATDbits.LATD10	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\HY27US08561A\HY27US08561A.h	67;"	d	line:67
NAND_CLE_TRIS::TRISDbits.TRISD10	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\HY27US08561A\HY27US08561A.h	66;"	d	line:66
NAND_COPYPROG_C1::0x00	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\HY27US08561A\HY27US08561A.h	93;"	d	line:93
NAND_COPYPROG_C2::0x8A	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\HY27US08561A\HY27US08561A.h	94;"	d	line:94
NAND_DATA::PMDIN1	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\HY27US08561A\HY27US08561A.h	74;"	d	line:74
NAND_PAGE_PER_BLOCK::32	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\HY27US08561A\HY27US08561A.h	105;"	d	line:105
NAND_PAGE_PROG_C1::0x80	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\HY27US08561A\HY27US08561A.h	91;"	d	line:91
NAND_PAGE_PROG_C2::0x10	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\HY27US08561A\HY27US08561A.h	92;"	d	line:92
NAND_PAGE_SIZE_BYTE::512	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\HY27US08561A\HY27US08561A.h	104;"	d	line:104
NAND_RB_PORT::PORTGbits.RG13	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\HY27US08561A\HY27US08561A.h	63;"	d	line:63
NAND_RB_TIMEOUT::2	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\HY27US08561A\HY27US08561A.h	115;"	d	line:115
NAND_RB_TRIS::TRISGbits.TRISG13	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\HY27US08561A\HY27US08561A.h	62;"	d	line:62
NAND_READ0::0x00	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\HY27US08561A\HY27US08561A.h	86;"	d	line:86
NAND_READ1::0x01	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\HY27US08561A\HY27US08561A.h	87;"	d	line:87
NAND_READ2::0x50	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\HY27US08561A\HY27US08561A.h	88;"	d	line:88
NAND_READSTATUS::0x70	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\HY27US08561A\HY27US08561A.h	97;"	d	line:97
NAND_READ_ID::0x90	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\HY27US08561A\HY27US08561A.h	89;"	d	line:89
NAND_RST::0xFF	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\HY27US08561A\HY27US08561A.h	90;"	d	line:90
NAND_RS_FAIL::1	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\HY27US08561A\HY27US08561A.h	114;"	d	line:114
NAND_RS_SUCCESS::0	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\HY27US08561A\HY27US08561A.h	113;"	d	line:113
NAND_WP_LAT::LATGbits.LATG14	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\HY27US08561A\HY27US08561A.h	71;"	d	line:71
NAND_WP_TRIS::TRISGbits.TRISG14	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\HY27US08561A\HY27US08561A.h	70;"	d	line:70
OUTPUT::0	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\HY27US08561A\HY27US08561A.h	77;"	d	line:77
PMPDelay::Nop;	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\HY27US08561A\HY27US08561A.h	248;"	d	line:248
SYSCLK::32000000	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\mainDemo.h	41;"	d	line:41
USE_AND_OR	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\HY27US08561A\HY27US08561A.c	39;"	d	line:39	file:
_HY27US08561A_H_	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\HY27US08561A\HY27US08561A.h	39;"	d	line:39
_MAINDEMO_H_	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\mainDemo.h	38;"	d	line:38
blockNum	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\HY27US08561A\HY27US08561A.c	186;"	l	line:186
blockPage	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\HY27US08561A\HY27US08561A.c	242;"	l	line:242
blockPage	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\HY27US08561A\HY27US08561A.c	299;"	l	line:299
dataBuffer	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\mainDemo.c	48;"	v	line:48
dataInput	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\mainDemo.c	46;"	v	line:46
getUART1	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\mainDemo.c	56;"	f	line:56	signature:(void)
i	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\HY27US08561A\HY27US08561A.c	242;"	l	line:242
i	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\HY27US08561A\HY27US08561A.c	299;"	l	line:299
id	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\HY27US08561A\HY27US08561A.c	106;"	l	line:106
j	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\mainDemo.c	45;"	v	line:45
main	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\mainDemo.c	62;"	f	line:62	signature:(void)
nandChkID	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\HY27US08561A\HY27US08561A.c	104;"	f	line:104	signature:(void)
nandChkID	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\HY27US08561A\HY27US08561A.h	155;"	p	line:155	signature:(void)
nandEraseBlk	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\HY27US08561A\HY27US08561A.c	184;"	f	line:184	signature:(INT16U block)
nandEraseBlk	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\HY27US08561A\HY27US08561A.h	199;"	p	line:199	signature:(INT16U block)
nandInit	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\HY27US08561A\HY27US08561A.c	55;"	f	line:55	signature:(void)
nandInit	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\HY27US08561A\HY27US08561A.h	136;"	p	line:136	signature:(void)
nandRdPage	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\HY27US08561A\HY27US08561A.c	297;"	f	line:297	signature:(INT16U block, INT16U page, INT16U col, INT8U* buffer)
nandRdPage	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\HY27US08561A\HY27US08561A.h	241;"	p	line:241	signature:(INT16U block, INT16U page, INT16U col, INT8U* buffer)
nandRdStatus	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\HY27US08561A\HY27US08561A.c	147;"	f	line:147	signature:(void)
nandRdStatus	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\HY27US08561A\HY27US08561A.h	176;"	p	line:176	signature:(void)
nandWrAddr::(addr)NAND_ALE_LAT=HIGH;NAND_D	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\HY27US08561A\HY27US08561A.h	277;"	d	line:277
nandWrCmd::(cmd)NAND_CLE_LAT=HIGH;NAND_DA	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\HY27US08561A\HY27US08561A.h	262;"	d	line:262
nandWrDat::(dat)NAND_DATA=dat;	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\HY27US08561A\HY27US08561A.h	292;"	d	line:292
nandWrPage	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\HY27US08561A\HY27US08561A.c	240;"	f	line:240	signature:(INT16U block, INT16U page, INT16U col, INT8U* buffer)
nandWrPage	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\HY27US08561A\HY27US08561A.h	223;"	p	line:223	signature:(INT16U block, INT16U page, INT16U col, INT8U* buffer)
putUART1	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\mainDemo.c	50;"	f	line:50	signature:(INT8U c)
status	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\HY27US08561A\HY27US08561A.c	149;"	l	line:149
status	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\HY27US08561A\HY27US08561A.c	187;"	l	line:187
status	D:\mcc30\projects\PIC24_Eval1\nandFlash Demo\HY27US08561A\HY27US08561A.c	243;"	l	line:243
